ALPHA Avro Canada CF-100 Canuck
Operation Procedures

Aircraft Weight, loaded: 34,889  lbs
Crew: 2

Adjust aircraft weight by selecting “Fuel and Payload” under the Aircraft menu.
__________________________________
BEFORE STARTING ENGINE

[ ] Brakes -- TEST and SET
[ ] Electrical Equipment -- OFF
[ ] Landing Gear Lever -- DOWN
[ ] Fuel Selector Valve -- BOTH
__________________________________
ENGINE START

Press Ctrl-E to initiate engine auto-start sequence.
___________________________________
BEFORE TAKEOFF

[ ] Brakes -- SET
[ ] Flight Controls -- FREE and CORRECT
[ ] Flight Instruments -- CHECK and SET
[ ] Fuel Quantity -- CHECK
[ ] Fuel Selector Valve -- RECHECK BOTH     
[ ] Elevator Trim -- NEUTRAL
[ ] Rudder Trim -- NEUTRAL

__________________________________
TAKEOFF

[ ] Flaps -- UP
[ ] Throttles -- FULL
[ ] Rotate --  125 KIAS
[ ] Liftoff – 140 KIAS
[ ] Brakes -- APPLY momentarily when airborne
[ ] Landing Gear -- UP
[ ] Flaps -- RETRACT

___________________________________
CLIMB

NORMAL CLIMB

[ ] Airspeed -- 240 KIAS
[ ] Throttle --  90% N1

__________________________________
DESCENT

[ ] Fuel Selector Valve -- ALL
[ ] Throttle -- AS DESIRED
[ ] Airbrake -- AS DESIRED
___________________________________
BEFORE LANDING (27184 lbs)

[ ] Approach speed -- 140 KIAS
[ ] Fuel Selector Valve – BEST
[ ] Flaps –- DOWN (below 170 KIAS)
[ ] Landing Gear –- DOWN (below 170 KIAS)
___________________________________
LANDING (27184 lbs)

[ ] Airspeed --  120 KIAS (flaps DOWN)
[ ] Flaps -- FULL DOWN (below 150 KIAS)
[ ] Trim – ADJUST
[ ] Over threshold – 120 KIAS
[ ] Flare to make contact at about 100 KIAS mph
[ ] Touchdown -- MAIN WHEELS FIRST
[ ] Landing Roll -- LOWER NOSE WHEEL GENTLY
[ ] Braking -- MINIMUM REQUIRED
___________________________________
AFTER LANDING

[ ] Flaps -- UP
___________________________________
BELLY LANDINGS and
WATER LANDINGS	(DITCHING)

[ ] Landing Gear -- UP
[ ] Landing Flaps -- DOWN
[ ] Shoulder Harness -- LOCKED
[ ] Canopy -- OPEN

PRIOR TO CONTACT WITH GROUND OR WATER

[ ] Switches -- OFF
[ ] Fuel Selector OFF
___________________________________
SECURING AIRPLANE

[ ] Brakes –- SET
[ ] Avionics -- OFF
[ ] Ignition Switches -- OFF
[ ] Master Battery Switch -- OFF
[ ] Fuel Selector Valve -- OFF
